"LAMMPS WWW Site"_lws - "LAMMPS Documentation"_ld - "LAMMPS Commands"_lc :c

:link(lws,http://lammps.sandia.gov)
:link(ld,Manual.html)
:link(lc,Commands_all.html)

:line

compute temp/uef command :h3

[Syntax:]

compute ID group-ID temp/uef :pre

ID, group-ID are documented in "compute"_compute.html command
temp/uef = style name of this compute command :ul

[Examples:]

compute 1 all temp/uef
compute 2 sel temp/uef :pre

[Description:]

This command is used to compute the kinetic energy tensor in
the reference frame of the applied flow field when
"fix nvt/uef"_fix_nh_uef.html or
"fix npt/uef"_fix_nh_uef.html is used.
It is not necessary to use this command to compute the scalar
value of the temperature. A "compute temp"_compute_temp.html
may be used for that purpose.

Output information for this command can be found in the
documentation for "compute temp"_compute_temp.html.

[Restrictions:]

This fix is part of the USER-UEF package. It is only enabled if LAMMPS
was built with that package. See the "Build
package"_Build_package.html doc page for more info.

This command can only be used when "fix nvt/uef"_fix_nh_uef.html
or "fix npt/uef"_fix_nh_uef.html is active.

[Related commands:]

"compute temp"_compute_temp.html,
"fix nvt/uef"_fix_nh_uef.html,
"compute pressure/uef"_compute_pressure_uef.html


[Default:] none
